(kicad_symbol_lib (version 20211014) (generator partreel-import)
  (symbol "SW_NKK_UB225SKG035F"
  		(pin_names
  			(offset 1.27)
  			(hide yes)
  		)
  		(exclude_from_sim no)
  		(in_bom yes)
  		(on_board yes)
  		(property "Reference" "SW"
  			(at 5.08 1.27 0)
  		)
  		(property "Value" "${FAMILY}"
  			(at 5.08 -2.032 0)
  		)
  		(property "Footprint" ""
  			(at 0 0 0)
  		)
  		(property "Datasheet" ""
  			(at 0 0 0)
  		)
  		(property "Description" "DPDT ON-(ON) Green Momentary Illuminated Pushbutton"
  			(at 0 0 0)
  		)
  		(symbol "SW_NKK_UB225SKG035F_1_0"
  			(text "GREEN"
  				(at 5.08 -23.368 0)
  			)
  			(pin bidirectional line
  				(at -5.08 -5.08 0)
  				(length 5.08)
  				(name "COM")
  				(number "1")
  			)
  			(pin bidirectional line
  				(at -5.08 -12.7 0)
  				(length 5.08)
  				(name "COM")
  				(number "4")
  			)
  			(pin input line
  				(at -5.08 -20.32 0)
  				(length 5.08)
  				(name "A")
  				(number "7")
  			)
  			(pin bidirectional line
  				(at 15.24 -2.54 180)
  				(length 5.08)
  				(name "NC")
  				(number "3")
  			)
  			(pin bidirectional line
  				(at 15.24 -7.62 180)
  				(length 5.08)
  				(name "NO")
  				(number "2")
  			)
  			(pin passive line
  				(at 15.24 -10.16 180)
  				(length 5.08)
  				(name "NC")
  				(number "6")
  			)
  			(pin passive line
  				(at 15.24 -15.24 180)
  				(length 5.08)
  				(name "NO")
  				(number "5")
  			)
  			(pin output line
  				(at 15.24 -20.32 180)
  				(length 5.08)
  				(name "C")
  				(number "8")
  			)
  		)
  		(embedded_fonts no)
  	)
)
