(footprint "SW_OMRON_A6SN-1101"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Body 4.48x7.5mm, 1 Way SPST Surface-Mounting Slide Switch With Flat Actuator (A6SN Series)")
	(property "Reference" "REF**"
		(at 0 -3.46496 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_OMRON_A6SN-1101"
		(at 0 3.46505 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(fp_text user "1"
		(at -3.2975 -1.90496 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "ON"
		(at 1.8778 -1.118897 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "ON"
		(at 2.4175 -0.889 270)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -4.125 0.00004)
		(size 2.15 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 4.125 0.00004)
		(size 2.15 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
