(footprint "SW_OMRON_B3U-3000PM"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Body 3.2x4.0mm, SPST Surface-Mounting Tactile Switch with Side Actuator (B3U Series)")
	(property "Reference" "REF**"
		(at -0.2875 -2.195 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_OMRON_B3U-3000PM"
		(at -0.2875 2.925 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at -1.7 0 180)
		(size 0.8 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 1.7 0 180)
		(size 0.8 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
