(footprint "SW_WURTH_461011220101"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Body 4.7x4.9mm, SPST-NO Switch Detector, Single Pole, Contact Rating")
	(property "Reference" "REF**"
		(at 0.2625 -3.425 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_WURTH_461011220101"
		(at 0.2625 3.425 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at 2.15 -1.2 180)
		(size 0.8 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 2.15 1.2 180)
		(size 0.8 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -2.15 -1.2 180)
		(size 0.8 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -2.15 1.2 180)
		(size 0.8 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
