(kicad_symbol_lib (version 20211014) (generator partreel-import)
  (symbol "XFMR_ANAREN_BD0205F5050A00"
  		(pin_names
  			(offset 1.27)
  		)
  		(exclude_from_sim no)
  		(in_bom yes)
  		(on_board yes)
  		(property "Reference" "TR"
  			(at 15.24 1.27 0)
  		)
  		(property "Value" "${VALUE}"
  			(at 15.24 -26.67 0)
  		)
  		(property "Footprint" ""
  			(at 0 0 0)
  		)
  		(property "Datasheet" ""
  			(at 0 0 0)
  		)
  		(property "Description" "70MHz - 1000MHz Ultra Low Profile Sub-Miniature Balanced to Unbalanced Transformer"
  			(at 0 0 0)
  		)
  		(symbol "XFMR_ANAREN_BD0205F5050A00_1_0"
  			(pin power_in line
  				(at -5.08 -2.54 0)
  				(length 5.08)
  				(name "GND")
  				(number "9")
  			)
  			(pin power_in line
  				(at -5.08 -5.08 0)
  				(length 5.08)
  				(name "GND")
  				(number "10")
  			)
  			(pin passive line
  				(at -5.08 -10.16 0)
  				(length 5.08)
  				(name "UNBAL")
  				(number "1")
  			)
  			(pin passive line
  				(at -5.08 -12.7 0)
  				(length 5.08)
  				(name "OPEN")
  				(number "2")
  			)
  			(pin power_in line
  				(at -5.08 -15.24 0)
  				(length 5.08)
  				(name "GND")
  				(number "3")
  			)
  			(pin power_in line
  				(at -5.08 -20.32 0)
  				(length 5.08)
  				(name "GND")
  				(number "4")
  			)
  			(pin power_in line
  				(at -5.08 -22.86 0)
  				(length 5.08)
  				(name "GND")
  				(number "5")
  			)
  			(pin passive line
  				(at 35.56 -2.54 180)
  				(length 5.08)
  				(name "BAL_P2")
  				(number "8")
  			)
  			(pin passive line
  				(at 35.56 -12.7 180)
  				(length 5.08)
  				(name "OPEN")
  				(number "7")
  			)
  			(pin passive line
  				(at 35.56 -22.86 180)
  				(length 5.08)
  				(name "BAL_P1")
  				(number "6")
  			)
  		)
  		(embedded_fonts no)
  	)
)
