(footprint "XFMR_CERN_HCR6BFW"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "CERN HF Current transformer")
	(property "Reference" "REF**"
		(at 0 -10.25 0)
		(layer "F.SilkS")
	)
	(property "Value" "XFMR_CERN_HCR6BFW"
		(at 0 10.25008 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_poly
		(pts
			(xy -5.50008 8.50009) (xy -5.50008 -8.5) (xy -5.50008 -8.59849) (xy -5.46165 -8.79167) (xy -5.38626 -8.97365) (xy -5.27682 -9.13743) (xy -5.13754 -9.2767) (xy -4.97375 -9.38613) (xy -4.79177 -9.4615) (xy -4.59858 -9.49992) (xy -4.50009 -9.49992) (xy -4.50009 -9.49993) (xy 4.49992 -9.49999) (xy 4.59841 -9.5) (xy 4.79161 -9.46157) (xy 4.9736 -9.38618) (xy 5.13738 -9.27675) (xy 5.27667 -9.13746) (xy 5.38611 -8.97367) (xy 5.46149 -8.79168) (xy 5.49992 -8.59849) (xy 5.49992 -8.5) (xy 5.49992 8.50008) (xy 5.49992 8.59857) (xy 5.46149 8.79177) (xy 5.38611 8.97375) (xy 5.27667 9.13754) (xy 5.13738 9.27683) (xy 4.9736 9.38627) (xy 4.79161 9.46165) (xy 4.59841 9.50008) (xy 4.49992 9.50008) (xy -4.50009 9.50008) (xy -4.59858 9.50008) (xy -4.79177 9.46165) (xy -4.97376 9.38627) (xy -5.13755 9.27683) (xy -5.27684 9.13755) (xy -5.38627 8.97376) (xy -5.46165 8.79177) (xy -5.50008 8.59858)
		)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_text user "19"
		(at -2.08672 2.73882 90)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "r1"
		(at 1.87361 7.66899 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "11"
		(at 0.79734 -5.08674 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -8.5 0)
		(size 5 6.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.1)
		(solder_paste_margin -4)
	)
	(pad "2" smd rect
		(at 8.5 0)
		(size 5 6.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.1)
		(solder_paste_margin -4)
	)
	(embedded_fonts no)
)
