(footprint "XFMR_CERN_HCRAMPO001"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "CERN HF Current transformer")
	(property "Reference" "REF**"
		(at 0 -10.25 0)
		(layer "F.SilkS")
	)
	(property "Value" "XFMR_CERN_HCRAMPO001"
		(at 0 10.25 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_poly
		(pts
			(xy -5.25 8.5) (xy -5.25 2.6) (xy -12 2.6) (xy -12.09849 2.6) (xy -12.29169 2.56157) (xy -12.47367 2.48618) (xy -12.63746 2.37674) (xy -12.77675 2.23746) (xy -12.88619 2.07367) (xy -12.96157 1.89168) (xy -13 1.69849) (xy -13 1.59999) (xy -13 -1.6) (xy -13 -1.6985) (xy -12.96157 -1.89169) (xy -12.88619 -2.07368) (xy -12.77675 -2.23747) (xy -12.63746 -2.37675) (xy -12.47367 -2.48619) (xy -12.29169 -2.56158) (xy -12.09849 -2.60001) (xy -12 -2.60001) (xy -5.25 -2.60001) (xy -5.25 -8.5) (xy -5.25 -8.5985) (xy -5.21156 -8.79169) (xy -5.13618 -8.97368) (xy -5.02674 -9.13747) (xy -4.88746 -9.27676) (xy -4.72367 -9.38619) (xy -4.54168 -9.46157) (xy -4.34849 -9.5) (xy -4.24999 -9.5) (xy 4.25 -9.5) (xy 4.34849 -9.5) (xy 4.54169 -9.46157) (xy 4.72368 -9.38619) (xy 4.88746 -9.27676) (xy 5.02675 -9.13747) (xy 5.13619 -8.97368) (xy 5.21157 -8.79169) (xy 5.25 -8.5985) (xy 5.25 -8.50001) (xy 5.25 -2.60001) (xy 12 -2.60001) (xy 12.09849 -2.60001) (xy 12.29169 -2.56158) (xy 12.47368 -2.48619) (xy 12.63746 -2.37675) (xy 12.77675 -2.23747) (xy 12.88619 -2.07368) (xy 12.96157 -1.89169) (xy 13 -1.6985) (xy 13 -1.6) (xy 13 1.59999) (xy 13 1.69849) (xy 12.96157 1.89168) (xy 12.88619 2.07367) (xy 12.77675 2.23746) (xy 12.63746 2.37674) (xy 12.47368 2.48618) (xy 12.29169 2.56157) (xy 12.09849 2.6) (xy 12 2.6) (xy 5.25 2.6) (xy 5.25 8.49999) (xy 5.25 8.59849) (xy 5.21157 8.79168) (xy 5.13619 8.97367) (xy 5.02675 9.13746) (xy 4.88746 9.27675) (xy 4.72368 9.38618) (xy 4.54169 9.46156) (xy 4.34849 9.49999) (xy 4.25 9.49999) (xy -4.24999 9.49999) (xy -4.34849 9.49999) (xy -4.54168 9.46156) (xy -4.72367 9.38618) (xy -4.88746 9.27675) (xy -5.02674 9.13746) (xy -5.13618 8.97367) (xy -5.21156 8.79168) (xy -5.25 8.59849) (xy -5.25 8.49999)
		)
		(fill no)
		(layer "Edge.Cuts")
	)
	(fp_text user "r1"
		(at 1.5875 7.425 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "10.5"
		(at 0 -5.14304 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "5.2"
		(at 6.35 1.075 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "26"
		(at -0.9525 -1.1475 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "19"
		(at -2.1 2.61115 90)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -17.5 0)
		(size 8 6.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.1)
		(solder_paste_margin -4)
	)
	(pad "2" smd rect
		(at 17.5 0)
		(size 8 6.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.1)
		(solder_paste_margin -4)
	)
	(embedded_fonts no)
)
