(kicad_symbol_lib (version 20211014) (generator partreel-import)
  (symbol "XFMR_CERN_HCRANQS"
  		(pin_names
  			(offset 1.27)
  			(hide yes)
  		)
  		(exclude_from_sim no)
  		(in_bom yes)
  		(on_board yes)
  		(property "Reference" "TR"
  			(at 5.08 1.27 0)
  		)
  		(property "Value" "${VALUE}"
  			(at 5.08 -24.13 0)
  		)
  		(property "Footprint" ""
  			(at 0 0 0)
  		)
  		(property "Datasheet" ""
  			(at 0 0 0)
  		)
  		(property "Description" "CERN R2E-DCDC ACF Power Transformer [48V; 12V]"
  			(at 0 0 0)
  		)
  		(symbol "XFMR_CERN_HCRANQS_1_0"
  			(text "NC"
  				(at 1.905 -3.81 900)
  			)
  			(text "NC"
  				(at 1.905 -16.51 900)
  			)
  			(text "CLIPS"
  				(at 5.08 -20.32 0)
  			)
  			(pin passive line
  				(at -5.08 -2.54 0)
  				(length 5.08)
  				(name "1")
  				(number "1")
  			)
  			(pin passive line
  				(at -5.08 -5.08 0)
  				(length 5.08)
  				(name "2")
  				(number "2")
  			)
  			(pin passive line
  				(at -5.08 -7.62 0)
  				(length 5.08)
  				(name "3")
  				(number "3")
  			)
  			(pin passive line
  				(at -5.08 -12.7 0)
  				(length 5.08)
  				(name "4")
  				(number "4")
  			)
  			(pin passive line
  				(at -5.08 -15.24 0)
  				(length 5.08)
  				(name "5")
  				(number "5")
  			)
  			(pin passive line
  				(at -5.08 -17.78 0)
  				(length 5.08)
  				(name "6")
  				(number "6")
  			)
  			(pin power_in line
  				(at -5.08 -20.32 0)
  				(length 5.08)
  				(name "13")
  				(number "13")
  			)
  			(pin passive line
  				(at 15.24 -2.54 180)
  				(length 5.08)
  				(name "12")
  				(number "12")
  			)
  			(pin passive line
  				(at 15.24 -5.08 180)
  				(length 5.08)
  				(name "11")
  				(number "11")
  			)
  			(pin passive line
  				(at 15.24 -7.62 180)
  				(length 5.08)
  				(name "10")
  				(number "10")
  			)
  			(pin passive line
  				(at 15.24 -12.7 180)
  				(length 5.08)
  				(name "9")
  				(number "9")
  			)
  			(pin passive line
  				(at 15.24 -15.24 180)
  				(length 5.08)
  				(name "8")
  				(number "8")
  			)
  			(pin passive line
  				(at 15.24 -17.78 180)
  				(length 5.08)
  				(name "7")
  				(number "7")
  			)
  			(pin power_in line
  				(at 15.24 -20.32 180)
  				(length 5.08)
  				(name "14")
  				(number "14")
  			)
  		)
  		(embedded_fonts no)
  	)
)
