(footprint "XFMR_PULSE_H1260NL"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "10/100BASE-T Transformer Modules, Body 7.11 x 12.7mm")
	(property "Reference" "REF**"
		(at 0 -7.32496 0)
		(layer "F.SilkS")
	)
	(property "Value" "XFMR_PULSE_H1260NL"
		(at 0 7.32505 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at -4.41 -4.44496)
		(size 1.46 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -4.41 -3.17496)
		(size 1.46 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -4.41 -1.90496)
		(size 1.46 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -4.41 -0.63496)
		(size 1.46 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -4.41 0.63504)
		(size 1.46 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -4.41 1.90504)
		(size 1.46 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -4.41 3.17505)
		(size 1.46 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -4.41 4.44505)
		(size 1.46 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 4.41 4.44505)
		(size 1.46 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 4.41 3.17505)
		(size 1.46 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 4.41 1.90504)
		(size 1.46 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 4.41 0.63504)
		(size 1.46 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 4.41 -0.63496)
		(size 1.46 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 4.41 -1.90496)
		(size 1.46 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 4.41 -3.17496)
		(size 1.46 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 4.41 -4.44496)
		(size 1.46 0.76)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
