(kicad_symbol_lib (version 20211014) (generator partreel-import)
  (symbol "XFMR_SCHAFFNER_IT243"
  		(pin_names
  			(offset 1.27)
  			(hide yes)
  		)
  		(exclude_from_sim no)
  		(in_bom yes)
  		(on_board yes)
  		(property "Reference" "TR"
  			(at 7.62 1.27 0)
  		)
  		(property "Value" "${VALUE}"
  			(at 7.62 -16.51 0)
  		)
  		(property "Footprint" ""
  			(at 0 0 0)
  		)
  		(property "Datasheet" ""
  			(at 0 0 0)
  		)
  		(property "Description" "Pulse Transformer with Double Secondary Winding IT313"
  			(at 0 0 0)
  		)
  		(symbol "XFMR_SCHAFFNER_IT243_1_0"
  			(text "PRI"
  				(at 1.27 -7.62 900)
  			)
  			(text "SEC"
  				(at 13.97 -7.62 900)
  			)
  			(pin passive line
  				(at -5.08 -5.08 0)
  				(length 5.08)
  				(name "PR_DOT")
  				(number "5")
  			)
  			(pin passive line
  				(at -5.08 -10.16 0)
  				(length 5.08)
  				(name "PR")
  				(number "6")
  			)
  			(pin passive line
  				(at 20.32 -2.54 180)
  				(length 5.08)
  				(name "SEC1_DOT")
  				(number "1")
  			)
  			(pin passive line
  				(at 20.32 -5.08 180)
  				(length 5.08)
  				(name "SEC2_DOT")
  				(number "3")
  			)
  			(pin passive line
  				(at 20.32 -10.16 180)
  				(length 5.08)
  				(name "SEC2")
  				(number "4")
  			)
  			(pin passive line
  				(at 20.32 -12.7 180)
  				(length 5.08)
  				(name "SEC1")
  				(number "2")
  			)
  		)
  		(embedded_fonts no)
  	)
)
