(kicad_symbol_lib (version 20211014) (generator partreel-import)
  (symbol "XFMR_TRIAD_CSE185L"
  		(pin_names
  			(offset 1.27)
  			(hide yes)
  		)
  		(exclude_from_sim no)
  		(in_bom yes)
  		(on_board yes)
  		(property "Reference" "TR"
  			(at 3.81 1.27 0)
  		)
  		(property "Value" "${VALUE}"
  			(at 3.81 -19.05 0)
  		)
  		(property "Footprint" ""
  			(at 0 0 0)
  		)
  		(property "Datasheet" ""
  			(at 0 0 0)
  		)
  		(property "Description" "50Hz/400Hz, Current Sense / Low Frequency Transformers 1:50 2A T/H"
  			(at 0 0 0)
  		)
  		(symbol "XFMR_TRIAD_CSE185L_1_0"
  			(pin passive line
  				(at -5.08 -2.54 0)
  				(length 5.08)
  				(name "2")
  				(number "2")
  			)
  			(pin passive line
  				(at -5.08 -7.62 0)
  				(length 5.08)
  				(name "3")
  				(number "3")
  			)
  			(pin passive line
  				(at -5.08 -12.7 0)
  				(length 5.08)
  				(name "1")
  				(number "1")
  			)
  			(pin passive line
  				(at -5.08 -15.24 0)
  				(length 5.08)
  				(name "4")
  				(number "4")
  			)
  			(pin passive line
  				(at 12.7 -2.54 180)
  				(length 5.08)
  				(name "8")
  				(number "8")
  			)
  			(pin passive line
  				(at 12.7 -7.62 180)
  				(length 5.08)
  				(name "5")
  				(number "5")
  			)
  			(pin passive line
  				(at 12.7 -12.7 180)
  				(length 5.08)
  				(name "7")
  				(number "7")
  			)
  			(pin passive line
  				(at 12.7 -15.24 180)
  				(length 5.08)
  				(name "6")
  				(number "6")
  			)
  		)
  		(embedded_fonts no)
  	)
)
