(footprint "XFMR_WURTH_EP7"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "WE-FB Flyback Transformer, Body 9.14 x 9.78mm, Size EP7")
	(property "Reference" "REF**"
		(at -0.515 -5.865 0)
		(layer "F.SilkS")
	)
	(property "Value" "XFMR_WURTH_EP7"
		(at -0.515 5.865 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at -4.065 3.735)
		(size 1.91 1.17)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -4.065 1.245)
		(size 1.91 1.17)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -4.065 -1.245)
		(size 1.91 1.17)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -4.065 -3.735)
		(size 1.91 1.17)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 4.065 -3.735)
		(size 1.91 1.17)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 4.065 -1.245)
		(size 1.91 1.17)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 4.065 1.245)
		(size 1.91 1.17)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 4.065 3.735)
		(size 1.91 1.17)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
